/*
 * Copyright (c) 2020 The ZMK Contributors
 *
 * SPDX-License-Identifier: MIT
 */

#include <dt-bindings/zmk/matrix_transform.h>

/ {
	chosen {
	    zmk,kscan = &kscan0;

	    zmk,matrix_transform = &default_transform;
	};

	/* 
	 * This transform correspondsto the 60% left without macro keypad and 65% right, even this
	 * combination of PCBs can have keys in different locations based on configuration.
	 */
	default_transform: keymap_transform_0 {
		compatible = "zmk,matrix-transform";
		columns = <14>;
		rows = <6>;
		map = <
RC(0,0) RC(0,1) RC(0,2) RC(0,3) RC(0,4) RC(0,5) RC(1,5)  /**/  RC(0,6) RC(0,7) RC(0,8) RC(0,9) RC(0,10) RC(0,11) RC(0,12) RC(0,13)
RC(1,0) RC(1,1) RC(1,2) RC(1,3) RC(1,4) RC(2,5)          /**/  RC(1,6) RC(1,7) RC(1,8) RC(1,9) RC(1,10) RC(1,11) RC(1,12) RC(1,13)
RC(2,0) RC(2,1) RC(2,2) RC(2,3) RC(2,4) RC(3,5)          /**/  RC(2,6) RC(2,7) RC(2,8) RC(2,9) RC(2,10) RC(2,11)          RC(2,13)
RC(3,0) RC(3,1) RC(3,2) RC(3,3) RC(3,4) RC(4,5)          /**/  RC(3,6) RC(3,7) RC(3,8) RC(3,9) RC(3,10) RC(3,11) RC(3,12) RC(3,13)
RC(4,0) RC(4,1) RC(4,2)         RC(4,4)                  /**/          RC(4,7) RC(4,8) RC(4,9)          RC(4,11) RC(4,12) RC(4,13)
		>;
	};
};
