# Controller

A debug console and configuration shield for serial TTL muxers. See the ```muxers``` folder for what connects to this shield.

## Hardware / BoM

| Item | Quantity | Unit Cost |
| ---- | -------- | --------- |
| [Keyboard FeatherWing (Keyboard + LCD)](https://www.tindie.com/products/arturo182/keyboard-featherwing-qwerty-keyboard-26-lcd/) | 1 | $55.00 |
| [Feather nRF52840 Express](https://www.adafruit.com/product/4062) | 1 | $24.95 |

## Libraries Used

### Local

These librarires are used by the project and contained in the ```src/``` folder local to the project.

- [GUIslice 0.15](https://github.com/ImpulseAdventure/GUIslice)
- [SdFat 1.1.4](https://github.com/greiman/SdFat)

### External

These libraries are used by the project and can be installed via the Arduino IDE library manager.

- [CircularBuffer](https://github.com/rlogiacco/CircularBuffer)
- [bbq10keyboard](https://github.com/arturo182/arduino_bbq10kbd)
- [Adafruit_ILI9341](https://github.com/adafruit/Adafruit_ILI9341)
- [Adafruit_NeoPixel](https://github.com/adafruit/Adafruit_NeoPixel)

## Hardware Docs

- [https://www.solder.party/docs/keyboard-featherwing/downloads/](https://www.solder.party/docs/keyboard-featherwing/downloads/)
- [https://github.com/arturo182/bbq10kbd_i2c_sw](https://github.com/arturo182/bbq10kbd_i2c_sw)
- [https://github.com/lvgl/lv_arduino](https://github.com/lvgl/lv_arduino)

## Implementation (Incomplete)

- Simple display of serial in/out via lcd
- Button for accessing symbols and control sequences via pop-up list that aren't on keyboard
- Button for accessing password selection pop-up to help with password entry over serial
  - This should be configured via a text file on the sd card
- Way to display pinouts stored on micro sd card
  - **YOU WILL NEED TO UPDATE THE CODE TO ADD NEW IMAGES**
  - Max number of files is 20
  - Max filename length is 24 (this includes the ```.``` and extension of the file)
  - The pinouts should be stored as bmp files *up to* 24 bit
  - Pinouts should be sized as close to 320x240 as possible
  - Pinouts should be stored at ```/pinouts``` on the root of the SD card
- Configuration read from muxes (if attached)

## Implementation (Complete)

- Battery level on feather neopixel (green = >80% ; yellow >=40% ; orange >= 25% ; red < 25%)
- User LED (red) always on when feather is running
- Battery level shown as progress bar in the upper right corner of the screen
- Config screen for Raspberry Pi UART/Speed
- SD card support (REQUIRED actually)
- SD Card information screen
- Keyboard setup
- 5 way switch for UI navigation instead of touch screen
- Button 4 as a way to switch between screens

## Building / Uploading

The ```make.ps1```, ```build.ps1``` and ```upload.ps1``` scripts can be used to build/upload this project. These scripts call the ```arduino-cli``` commands programatically.
