Archive member included to satisfy reference by file (symbol)

C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                              (Reset_Handler)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o (delay)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o) (yield)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o) (SystemInit)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o (SystemCoreClock)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o) (analogReference)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o (pinMode)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o (pinPeripheral)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o) (tickReset)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o (SERCOM::SERCOM(Sercom*))
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o (Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad))
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o (main)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o) (Print::write(unsigned char const*, unsigned int))
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o) (USBDeviceClass::init())
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__cxa_pure_virtual)
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o) (operator new(unsigned int))
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o) (CDC_GetInterface(unsigned char*))
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o) (PluggableUSB_::getInterface(unsigned char*))
C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o) (USBDevice_SAMD21G18x::reset())
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_uqi.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o) (__gnu_thumb1_case_uqi)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o (__aeabi_uidiv)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o) (__aeabi_idiv)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o) (__aeabi_idiv0)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_dcmplt)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_d2uiz)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_dadd)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_ddiv)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o) (__eqdf2)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o) (__gedf2)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o) (__ledf2)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_dmul)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_dsub)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_dcmpun)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o) (__aeabi_d2iz)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (__aeabi_ui2d)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_clzsi2.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o) (__clzsi2)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o (exit)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o) (_global_impure_ptr)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o (__libc_init_array)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o) (malloc)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o) (memcpy)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o (memset)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o) (_free_r)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o) (_malloc_r)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o) (_sbrk_r)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-strlen.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (strlen)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o) (vsnprintf)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o) (__malloc_lock)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o) (_svfprintf_r)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o) (_printf_i)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o) (errno)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o) (__retarget_lock_acquire_recursive)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o) (memchr)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o) (memmove)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o) (_realloc_r)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o) (_malloc_usable_size_r)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_shi.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o) (__gnu_thumb1_case_shi)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o) (_sbrk)
c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o) (_exit)

Allocating common symbols
Common symbol       size              file

__lock___atexit_recursive_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___arc4random_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
errno               0x4               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
__lock___env_recursive_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___sinit_recursive_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___malloc_recursive_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___at_quick_exit_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___dd_hash_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___tz_mutex   0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___sfp_recursive_mutex
                    0x1               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)

Discarded input sections

 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
 .data          0x00000000        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
 .text          0x00000000       0x78 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
 .ARM.extab     0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
 .ARM.exidx     0x00000000        0x8 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
 .ARM.attributes
                0x00000000       0x1b c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .text._Z14timerIsSyncingv
                0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .text._Z12timerDisablev
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .data.g_apTCInstances
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .text.millis   0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .text.__halt   0x00000000        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .text.analogReadResolution
                0x00000000       0x4c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .text.analogWriteResolution
                0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .text.analogRead
                0x00000000       0xe8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .text.analogWrite
                0x00000000      0x1cc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .rodata        0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .bss.tcEnabled.12735
                0x00000000        0x6 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .data._ADCResolution
                0x00000000        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .data._readResolution
                0x00000000        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .data._writeResolution
                0x00000000        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .text.digitalRead
                0x00000000       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM25isBufferOverflowErrorUARTEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM17isParityErrorUARTEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM8resetSPIEv
                0x00000000       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM9enableSPIEv
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM10disableSPIEv
                0x00000000       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15setDataOrderSPIE15SercomDataOrder
                0x00000000       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15getDataOrderSPIEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15setClockModeSPIE18SercomSpiClockMode
                0x00000000       0x40 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15transferDataSPIEh
                0x00000000       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM24isBufferOverflowErrorSPIEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM22isDataRegisterEmptySPIEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM28calculateBaudrateSynchronousEm
                0x00000000       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM12initSPIClockE18SercomSpiClockModem
                0x00000000       0x26 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14setBaudrateSPIEh
                0x00000000       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM9resetWIREEv
                0x00000000       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM10enableWIREEv
                0x00000000       0x2a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM11disableWIREEv
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM18prepareNackBitWIREEv
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM17prepareAckBitWIREEv
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM22prepareCommandBitsWireEh
                0x00000000       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM21startTransmissionWIREEh23SercomWireReadWriteFlag
                0x00000000       0x7c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM18sendDataMasterWIREEh
                0x00000000       0x26 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM17sendDataSlaveWIREEh
                0x00000000       0x1e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM12isMasterWIREEv
                0x00000000       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM11isSlaveWIREEv
                0x00000000       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13isBusIdleWIREEv
                0x00000000       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14isBusOwnerWIREEv
                0x00000000       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM16isBusUnknownWIREEv
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13isArbLostWIREEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13isBusBusyWIREEv
                0x00000000       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM15isDataReadyWIREEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM18isStopDetectedWIREEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM21isRestartDetectedWIREEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14isAddressMatchEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM25isMasterReadOperationWIREEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM20isRXNackReceivedWIREEv
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13availableWIREEv
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM12readDataWIREEv
                0x00000000       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM7initSPIE14SercomSpiTXPad11SercomRXPad17SercomSpiCharSize15SercomDataOrder
                0x00000000       0x52 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM13initSlaveWIREEhb
                0x00000000       0x4a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .text._ZN6SERCOM14initMasterWIREEm
                0x00000000       0x54 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .group         0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .text._ZN4Uart16extractNbStopBitEt
                0x00000000        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .text._ZN4UartC2EP6SERCOMhh11SercomRXPad15SercomUartTXPadhh
                0x00000000       0x80 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .group         0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print17availableForWriteEv
                0x00000000        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5flushEv
                0x00000000        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5writeEPKc
                0x00000000       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEPK19__FlashStringHelper
                0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printERK6String
                0x00000000        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEPKc
                0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEc
                0x00000000        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printERK9Printable
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .rodata._ZN5Print7printlnEv.str1.1
                0x00000000        0x3 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEv
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEPK19__FlashStringHelper
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnERK6String
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEPKc
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEc
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnERK9Printable
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print6printfEPKcz
                0x00000000       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print11printNumberEmh
                0x00000000       0x50 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEli
                0x00000000       0x3e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEii
                0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEii
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEli
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEmi
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEhi
                0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEhi
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEji
                0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEji
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEmi
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .rodata._ZN5Print10printFloatEdh.str1.1
                0x00000000        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print10printFloatEdh
                0x00000000      0x168 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print5printEdi
                0x00000000        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .text._ZN5Print7printlnEdi
                0x00000000       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .rodata._ZTV5Print
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .group         0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass7standbyEv
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass6detachEv
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass3endEv
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass10configuredEv
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass10setHandlerEmP9EPHandler
                0x00000000        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass5stallEm
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass9connectedEv
                0x00000000       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass12packMessagesEb
                0x00000000       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN14USBDeviceClass7sendZlpEm
                0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .text.__cxa_pure_virtual
                0x00000000        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .text.__cxa_deleted_virtual
                0x00000000        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_info    0x00000000     0x1033 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_abbrev  0x00000000      0x2af C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_aranges
                0x00000000       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_ranges  0x00000000       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_line    0x00000000      0x42f C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_str     0x00000000      0x7d5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .comment       0x00000000       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .debug_frame   0x00000000       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .ARM.attributes
                0x00000000       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .text._Znaj    0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .text._ZdaPv   0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._Z17_CDC_GetInterfacev
                0x00000000        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._Z23_CDC_GetInterfaceLengthv
                0x00000000        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._ZN7Serial_5beginEm
                0x00000000        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._ZN7Serial_5beginEmh
                0x00000000        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._ZN7Serial_3endEv
                0x00000000       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._ZN7Serial_9readBytesEPcj
                0x00000000       0x3c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._ZN7Serial_cvbEv
                0x00000000       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .text._ZN13PluggableUSB_12getShortNameEPc
                0x00000000       0x1e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .text._ZN13PluggableUSB_4plugEP18PluggableUSBModule
                0x00000000       0x58 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .text._ZN13PluggableUSB_C2Ev
                0x00000000       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .text          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
 .data          0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
 .bss           0x00000000        0x0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_uqi.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_uqi.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
 .text          0x00000000      0x1d4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
 .debug_frame   0x00000000       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
 .ARM.attributes
                0x00000000       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
 .text          0x00000000       0x7c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
 .ARM.attributes
                0x00000000       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
 .text          0x00000000       0x3c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
 .debug_frame   0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
 .text          0x00000000      0x6d4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
 .debug_frame   0x00000000       0x38 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
 .text          0x00000000      0x5d0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
 .rodata        0x00000000       0x40 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
 .debug_frame   0x00000000       0x3c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
 .text          0x00000000       0x78 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
 .debug_frame   0x00000000       0x38 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
 .text          0x00000000       0xe4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
 .debug_frame   0x00000000       0x38 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
 .text          0x00000000       0xe0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
 .debug_frame   0x00000000       0x38 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
 .text          0x00000000      0x4d8 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
 .rodata        0x00000000       0x40 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
 .debug_frame   0x00000000       0x3c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
 .text          0x00000000      0x724 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
 .debug_frame   0x00000000       0x3c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
 .text          0x00000000       0x3c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
 .debug_frame   0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
 .text          0x00000000       0x6c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
 .debug_frame   0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
 .text          0x00000000       0x4c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
 .debug_frame   0x00000000       0x28 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
 .text          0x00000000       0x3c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_clzsi2.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_clzsi2.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_clzsi2.o)
 .ARM.attributes
                0x00000000       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_clzsi2.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
 .text.exit     0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
 .debug_frame   0x00000000       0x28 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
 .rodata._global_impure_ptr
                0x00000000        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-strlen.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-strlen.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .text._vsnprintf_r
                0x00000000       0x56 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .text.vsnprintf
                0x00000000       0x18 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .debug_frame   0x00000000       0x48 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .text.__ssputs_r
                0x00000000       0xc4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .text.__ssprint_r
                0x00000000      0x100 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .rodata._svfprintf_r.str1.1
                0x00000000       0x11 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .text._svfprintf_r
                0x00000000      0x200 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .debug_frame   0x00000000       0x74 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .text._printf_common
                0x00000000       0xde c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .rodata._printf_i.str1.1
                0x00000000       0x22 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .text._printf_i
                0x00000000      0x224 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .debug_frame   0x00000000       0x54 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .text.cleanup_glue
                0x00000000       0x1a c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .text._reclaim_reent
                0x00000000       0xcc c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_init
                0x00000000        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_init_recursive
                0x00000000        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_close
                0x00000000        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_close_recursive
                0x00000000        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_acquire
                0x00000000        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_try_acquire
                0x00000000        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_try_acquire_recursive
                0x00000000        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text.__retarget_lock_release
                0x00000000        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
 .text.memchr   0x00000000       0x16 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
 .debug_frame   0x00000000       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
 .text.memmove  0x00000000       0x26 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
 .debug_frame   0x00000000       0x28 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
 .text._realloc_r
                0x00000000       0x4c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
 .debug_frame   0x00000000       0x30 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
 .text._malloc_usable_size_r
                0x00000000       0x10 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
 .debug_frame   0x00000000       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
 .text          0x00000000       0x14 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_shi.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_shi.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_shi.o)
 .ARM.attributes
                0x00000000       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_shi.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
 .text._exit    0x00000000        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
 .debug_frame   0x00000000       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
 .ARM.attributes
                0x00000000       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtend.o
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtend.o
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtend.o
 .text          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o
 .data          0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o
 .bss           0x00000000        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o

Memory Configuration

Name             Origin             Length             Attributes
FLASH            0x00002000         0x0003e000         xr
RAM              0x20000000         0x00008000         xrw
*default*        0x00000000         0xffffffff

Linker script and memory map

LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
LOAD C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
LOAD C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
START GROUP
LOAD C:\Users\mcros\AppData\Local\Arduino15\packages\adafruit\tools\CMSIS\5.4.0/CMSIS/Lib/GCC/\libarm_cortexM0l_math.a
LOAD C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a
END GROUP
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libstdc++_nano.a
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libm.a
START GROUP
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a
END GROUP
START GROUP
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a
END GROUP
START GROUP
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a
END GROUP
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtend.o
LOAD c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o

.text           0x00002000     0x2b14
                0x00002000                __text_start__ = .
 *(.sketch_boot)
                0x00002000                . = ALIGN (0x2000)
 *(.isr_vector)
 .isr_vector    0x00002000       0xb4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                0x00002000                exception_table
 *(.text*)
 .text          0x000020b4       0x48 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
 .text.SERCOM4_Handler
                0x000020fc       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x000020fc                SERCOM4_Handler
 .text.SERCOM3_Handler
                0x0000210c       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x0000210c                SERCOM3_Handler
 .text.loop     0x0000211c       0x24 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x0000211c                loop
 .text.TC5_Handler
                0x00002140       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x00002140                TC5_Handler
 .text._Z17timerStartCounterv
                0x00002170       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x00002170                timerStartCounter()
 .text._Z10timerResetv
                0x00002188       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x00002188                timerReset()
 .text._Z14timerConfigurei
                0x000021a4       0x98 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x000021a4                timerConfigure(int)
 .text.setup    0x0000223c       0x38 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x0000223c                setup
 .text.startup._GLOBAL__sub_I_uartBuffer
                0x00002274       0x58 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .text.SERCOM0_Handler
                0x000022cc       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x000022cc                SERCOM0_Handler
 .text.SERCOM5_Handler
                0x000022dc       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x000022dc                SERCOM5_Handler
 .text.startup._GLOBAL__sub_I_g_APinDescription
                0x000022ec       0x94 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .text.Dummy_Handler
                0x00002380        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                0x00002380                DMAC_Handler
                0x00002380                HardFault_Handler
                0x00002380                AC_Handler
                0x00002380                PendSV_Handler
                0x00002380                NMI_Handler
                0x00002380                TC7_Handler
                0x00002380                SERCOM1_Handler
                0x00002380                ADC_Handler
                0x00002380                TCC1_Handler
                0x00002380                SERCOM2_Handler
                0x00002380                TCC0_Handler
                0x00002380                RTC_Handler
                0x00002380                EIC_Handler
                0x00002380                TC6_Handler
                0x00002380                WDT_Handler
                0x00002380                TC4_Handler
                0x00002380                TC3_Handler
                0x00002380                Dummy_Handler
                0x00002380                PM_Handler
                0x00002380                SVC_Handler
                0x00002380                TCC2_Handler
                0x00002380                EVSYS_Handler
                0x00002380                I2S_Handler
                0x00002380                NVMCTRL_Handler
                0x00002380                DAC_Handler
                0x00002380                PTC_Handler
                0x00002380                SYSCTRL_Handler
 *fill*         0x00002382        0x2 
 .text.USB_Handler
                0x00002384       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                0x00002384                USB_Handler
 .text.Reset_Handler
                0x00002398       0x54 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                0x00002398                Reset_Handler
 .text.SysTick_Handler
                0x000023ec       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                0x000023ec                SysTick_Handler
 .text.USB_SetHandler
                0x000023fc        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                0x000023fc                USB_SetHandler
 .text.micros   0x00002408       0x60 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                0x00002408                micros
 .text.delay    0x00002468       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                0x00002468                delay
 .text.SysTick_DefaultHandler
                0x00002494       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                0x00002494                SysTick_DefaultHandler
 .text.__empty  0x000024a8        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
                0x000024a8                yield
 .text.__false  0x000024aa        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
                0x000024aa                sysTickHook
 *fill*         0x000024ae        0x2 
 .text.SystemInit
                0x000024b0      0x160 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
                0x000024b0                SystemInit
 .text.init     0x00002610       0xe0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                0x00002610                init
 .text.analogReference
                0x000026f0       0x88 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                0x000026f0                analogReference
 .text.pinMode  0x00002778       0x60 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                0x00002778                pinMode
 .text.digitalWrite
                0x000027d8       0x58 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                0x000027d8                digitalWrite
 .text.pinPeripheral
                0x00002830       0xbc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
                0x00002830                pinPeripheral
 .text.initiateReset
                0x000028ec        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                0x000028ec                initiateReset
 .text.cancelReset
                0x000028f8       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                0x000028f8                cancelReset
 .text.tickReset
                0x00002908       0x74 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                0x00002908                tickReset
 .text._ZN6SERCOMC2EP6Sercom
                0x0000297c        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x0000297c                SERCOM::SERCOM(Sercom*)
                0x0000297c                SERCOM::SERCOM(Sercom*)
 .text._ZN6SERCOM9initFrameE18SercomUartCharSize15SercomDataOrder16SercomParityMode19SercomNumberStopBit
                0x00002980       0x3a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002980                SERCOM::initFrame(SercomUartCharSize, SercomDataOrder, SercomParityMode, SercomNumberStopBit)
 .text._ZN6SERCOM8initPadsE15SercomUartTXPad11SercomRXPad
                0x000029ba       0x26 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x000029ba                SERCOM::initPads(SercomUartTXPad, SercomRXPad)
 .text._ZN6SERCOM9resetUARTEv
                0x000029e0       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x000029e0                SERCOM::resetUART()
 .text._ZN6SERCOM10enableUARTEv
                0x000029fa       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x000029fa                SERCOM::enableUART()
 .text._ZN6SERCOM9flushUARTEv
                0x00002a0e       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a0e                SERCOM::flushUART()
 .text._ZN6SERCOM15clearStatusUARTEv
                0x00002a1e        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a1e                SERCOM::clearStatusUART()
 .text._ZN6SERCOM17availableDataUARTEv
                0x00002a26        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a26                SERCOM::availableDataUART()
 .text._ZN6SERCOM11isUARTErrorEv
                0x00002a30        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a30                SERCOM::isUARTError()
 .text._ZN6SERCOM20acknowledgeUARTErrorEv
                0x00002a38        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a38                SERCOM::acknowledgeUARTError()
 .text._ZN6SERCOM16isFrameErrorUARTEv
                0x00002a46        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a46                SERCOM::isFrameErrorUART()
 .text._ZN6SERCOM19clearFrameErrorUARTEv
                0x00002a50        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a50                SERCOM::clearFrameErrorUART()
 .text._ZN6SERCOM23isDataRegisterEmptyUARTEv
                0x00002a5c        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a5c                SERCOM::isDataRegisterEmptyUART()
 .text._ZN6SERCOM12readDataUARTEv
                0x00002a66        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a66                SERCOM::readDataUART()
 .text._ZN6SERCOM13writeDataUARTEh
                0x00002a6e       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a6e                SERCOM::writeDataUART(unsigned char)
 .text._ZN6SERCOM36enableDataRegisterEmptyInterruptUARTEv
                0x00002a7e        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a7e                SERCOM::enableDataRegisterEmptyInterruptUART()
 .text._ZN6SERCOM37disableDataRegisterEmptyInterruptUARTEv
                0x00002a86        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a86                SERCOM::disableDataRegisterEmptyInterruptUART()
 *fill*         0x00002a8e        0x2 
 .text._ZN6SERCOM14getSercomIndexEv
                0x00002a90       0x5c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002a90                SERCOM::getSercomIndex()
 .text._ZN6SERCOM13initClockNVICEv
                0x00002aec       0x90 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002aec                SERCOM::initClockNVIC()
 .text._ZN6SERCOM8initUARTE14SercomUartMode20SercomUartSampleRatem
                0x00002b7c       0x6c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                0x00002b7c                SERCOM::initUART(SercomUartMode, SercomUartSampleRate, unsigned long)
 .text._ZN4UartcvbEv
                0x00002be8        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002be8                Uart::operator bool()
 .text._ZN4Uart5beginEm
                0x00002bec       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002bec                Uart::begin(unsigned long)
 .text._ZN4Uart4peekEv
                0x00002bfc       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002bfc                Uart::peek()
 .text._ZN4Uart3endEv
                0x00002c16       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002c16                Uart::end()
 .text._ZN4Uart15extractCharSizeEt
                0x00002c36       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002c36                Uart::extractCharSize(unsigned short)
 .text._ZN4Uart13extractParityEt
                0x00002c5e       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002c5e                Uart::extractParity(unsigned short)
 *fill*         0x00002c72        0x2 
 .text._ZN4Uart5beginEmt
                0x00002c74       0xf8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002c74                Uart::begin(unsigned long, unsigned short)
 .text._ZN11RingBufferNILi256EEC2Ev
                0x00002d6c       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002d6c                RingBufferN<256>::RingBufferN()
                0x00002d6c                RingBufferN<256>::RingBufferN()
 .text._ZN4UartC2EP6SERCOMhh11SercomRXPad15SercomUartTXPad
                0x00002d88       0x70 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002d88                Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad)
                0x00002d88                Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad)
 .text._ZN11RingBufferNILi256EE9availableEv
                0x00002df8       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002df8                RingBufferN<256>::available()
 .text._ZN4Uart5flushEv
                0x00002e0a       0x1a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002e0a                Uart::flush()
 .text._ZN4Uart9availableEv
                0x00002e24        0xa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002e24                Uart::available()
 .text._ZN11RingBufferNILi256EE17availableForStoreEv
                0x00002e2e       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002e2e                RingBufferN<256>::availableForStore()
 .text._ZN4Uart17availableForWriteEv
                0x00002e4e        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002e4e                Uart::availableForWrite()
 .text._ZN4Uart10IrqHandlerEv
                0x00002e5a       0xcc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002e5a                Uart::IrqHandler()
 *fill*         0x00002f26        0x2 
 .text._ZN4Uart5writeEh
                0x00002f28       0xb4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002f28                Uart::write(unsigned char)
 .text._ZN4Uart4readEv
                0x00002fdc       0x4c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00002fdc                Uart::read()
 .text._Z11initVariantv
                0x00003028        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                0x00003028                initVariant()
 *fill*         0x0000302a        0x2 
 .text.startup.main
                0x0000302c       0x44 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                0x0000302c                main
 .text._ZN5Print5writeEPKhj
                0x00003070       0x24 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
                0x00003070                Print::write(unsigned char const*, unsigned int)
 .text._ZN26DoubleBufferedEPOutHandler4initEv
                0x00003094        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003094                DoubleBufferedEPOutHandler::init()
 .text._ZL5utox8mPc
                0x00003096       0x26 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN26DoubleBufferedEPOutHandlerD2Ev
                0x000030bc       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000030bc                DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler()
                0x000030bc                DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler()
 .text._ZN26DoubleBufferedEPOutHandlerD0Ev
                0x000030d0       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000030d0                DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler()
 *fill*         0x000030e2        0x2 
 .text._ZN14USBDeviceClass6initEPEmm.part.0
                0x000030e4       0xe8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._ZN7__GuardC2Ev
                0x000031cc        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000031cc                __Guard::__Guard()
                0x000031cc                __Guard::__Guard()
 .text._ZN7__GuardD2Ev
                0x000031da        0xe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000031da                __Guard::~__Guard()
                0x000031da                __Guard::~__Guard()
 .text._ZNK26DoubleBufferedEPOutHandler9availableEv
                0x000031e8       0x5e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000031e8                DoubleBufferedEPOutHandler::available() const
 *fill*         0x00003246        0x2 
 .text._ZN26DoubleBufferedEPOutHandler7releaseEv
                0x00003248       0x54 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003248                DoubleBufferedEPOutHandler::release()
 .text._ZN26DoubleBufferedEPOutHandler4recvEPvm
                0x0000329c      0x11a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x0000329c                DoubleBufferedEPOutHandler::recv(void*, unsigned long)
 .text._ZN26DoubleBufferedEPOutHandler14handleEndpointEv
                0x000033b6       0xc2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000033b6                DoubleBufferedEPOutHandler::handleEndpoint()
 .text._ZN14USBDeviceClass14SendInterfacesEPm
                0x00003478       0x2e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003478                USBDeviceClass::SendInterfaces(unsigned long*)
 *fill*         0x000034a6        0x2 
 .text._ZN14USBDeviceClass14handleEndpointEh
                0x000034a8       0x44 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000034a8                USBDeviceClass::handleEndpoint(unsigned char)
 .text._ZN14USBDeviceClass4initEv
                0x000034ec       0xf0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000034ec                USBDeviceClass::init()
 .text._ZN14USBDeviceClass6attachEv
                0x000035dc       0x34 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000035dc                USBDeviceClass::attach()
 .text._ZN14USBDeviceClass10setAddressEm
                0x00003610       0x44 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003610                USBDeviceClass::setAddress(unsigned long)
 .text._ZN14USBDeviceClass25handleClassInterfaceSetupER8USBSetup
                0x00003654       0x44 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003654                USBDeviceClass::handleClassInterfaceSetup(USBSetup&)
 .text._ZN14USBDeviceClass6initEPEmm
                0x00003698       0xec C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003698                USBDeviceClass::initEP(unsigned long, unsigned long)
 .text._ZN14USBDeviceClass13initEndpointsEv
                0x00003784       0x24 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003784                USBDeviceClass::initEndpoints()
 .text._ZN14USBDeviceClass9availableEm
                0x000037a8       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000037a8                USBDeviceClass::available(unsigned long)
 .text._ZN14USBDeviceClass5flushEm
                0x000037d4       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000037d4                USBDeviceClass::flush(unsigned long)
 .text._ZN14USBDeviceClass14armRecvCtrlOUTEm
                0x00003800       0x5c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003800                USBDeviceClass::armRecvCtrlOUT(unsigned long)
 .text._ZN14USBDeviceClass11recvControlEPvm
                0x0000385c       0x3c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x0000385c                USBDeviceClass::recvControl(void*, unsigned long)
 .text._ZN14USBDeviceClass7armRecvEm
                0x00003898       0x38 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003898                USBDeviceClass::armRecv(unsigned long)
 .text._ZN14USBDeviceClass4recvEmPvm
                0x000038d0       0xd8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000038d0                USBDeviceClass::recv(unsigned long, void*, unsigned long)
 .text._ZN14USBDeviceClass4recvEm
                0x000039a8       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000039a8                USBDeviceClass::recv(unsigned long)
 .text._ZN14USBDeviceClass4sendEmPKvm
                0x000039c4      0x110 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x000039c4                USBDeviceClass::send(unsigned long, void const*, unsigned long)
 .text._ZN14USBDeviceClass7armSendEmPKvm
                0x00003ad4       0x48 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003ad4                USBDeviceClass::armSend(unsigned long, void const*, unsigned long)
 .text._ZN14USBDeviceClass11sendControlEPKvm
                0x00003b1c       0x54 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003b1c                USBDeviceClass::sendControl(void const*, unsigned long)
 .text._ZN14USBDeviceClass20sendStringDescriptorEPKhh
                0x00003b70       0x68 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003b70                USBDeviceClass::sendStringDescriptor(unsigned char const*, unsigned char)
 .text._ZN14USBDeviceClass17sendConfigurationEm
                0x00003bd8       0x80 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003bd8                USBDeviceClass::sendConfiguration(unsigned long)
 .text._ZN14USBDeviceClass14sendDescriptorER8USBSetup
                0x00003c58       0xe4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003c58                USBDeviceClass::sendDescriptor(USBSetup&)
 .text._ZN14USBDeviceClass19handleStandardSetupER8USBSetup
                0x00003d3c      0x118 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003d3c                USBDeviceClass::handleStandardSetup(USBSetup&)
 .text._ZN14USBDeviceClass10ISRHandlerEv
                0x00003e54      0x150 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003e54                USBDeviceClass::ISRHandler()
 .text.UDD_Handler
                0x00003fa4       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00003fa4                UDD_Handler
 .text.startup._GLOBAL__sub_I_usbd
                0x00003fb4       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .text._Znwj    0x00003fc4        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                0x00003fc4                operator new(unsigned int)
 .text._ZdlPv   0x00003fcc        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                0x00003fcc                operator delete(void*)
 .text._ZN7Serial_17availableForWriteEv
                0x00003fd4        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00003fd4                Serial_::availableForWrite()
 .text._ZN7Serial_5writeEh
                0x00003fd8       0x14 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00003fd8                Serial_::write(unsigned char)
 .text._ZN7Serial_9availableEv
                0x00003fec        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00003fec                Serial_::available()
 .text._ZN7Serial_5flushEv
                0x00003ff8        0xc C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00003ff8                Serial_::flush()
 .text._ZN7Serial_5writeEPKhj
                0x00004004       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00004004                Serial_::write(unsigned char const*, unsigned int)
 .text._ZN7Serial_4peekEv
                0x00004030       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00004030                Serial_::peek()
 .text._ZN7Serial_4readEv
                0x0000404c       0x24 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x0000404c                Serial_::read()
 .text._Z16CDC_GetInterfacePh
                0x00004070       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00004070                CDC_GetInterface(unsigned char*)
 .text._Z9CDC_SetupR8USBSetup
                0x0000408c       0x7c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x0000408c                CDC_Setup(USBSetup&)
 .text.startup._GLOBAL__sub_I__Z17_CDC_GetInterfacev
                0x00004108       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .text._ZN13PluggableUSB_12getInterfaceEPh
                0x00004130       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                0x00004130                PluggableUSB_::getInterface(unsigned char*)
 .text._ZN13PluggableUSB_13getDescriptorER8USBSetup
                0x00004158       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                0x00004158                PluggableUSB_::getDescriptor(USBSetup&)
 .text._ZN13PluggableUSB_5setupER8USBSetup
                0x00004178       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                0x00004178                PluggableUSB_::setup(USBSetup&)
 .text._Z12PluggableUSBv
                0x00004198       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                0x00004198                PluggableUSB()
 .text._ZN20USBDevice_SAMD21G18x5resetEv
                0x000041c0       0x2a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                0x000041c0                USBDevice_SAMD21G18x::reset()
 *fill*         0x000041ea        0x2 
 .text._ZN20USBDevice_SAMD21G18x9calibrateEv
                0x000041ec       0x60 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                0x000041ec                USBDevice_SAMD21G18x::calibrate()
 .text          0x0000424c       0x14 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_uqi.o)
                0x0000424c                __gnu_thumb1_case_uqi
 .text          0x00004260      0x114 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
                0x00004260                __aeabi_uidiv
                0x00004260                __udivsi3
                0x0000436c                __aeabi_uidivmod
 .text          0x00004374        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
                0x00004374                __aeabi_idiv0
                0x00004374                __aeabi_ldiv0
 .text.__libc_init_array
                0x00004378       0x48 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
                0x00004378                __libc_init_array
 .text.malloc   0x000043c0       0x14 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
                0x000043c0                malloc
 .text.free     0x000043d4       0x14 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
                0x000043d4                free
 .text.memcpy   0x000043e8       0x12 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
                0x000043e8                memcpy
 .text.memset   0x000043fa       0x10 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
                0x000043fa                memset
 *fill*         0x0000440a        0x2 
 .text._free_r  0x0000440c       0x94 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
                0x0000440c                _free_r
 .text._malloc_r
                0x000044a0       0xbc c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                0x000044a0                _malloc_r
 .text._sbrk_r  0x0000455c       0x24 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
                0x0000455c                _sbrk_r
 .text          0x00004580        0xe c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-strlen.o)
                0x00004580                strlen
 *fill*         0x0000458e        0x2 
 .text.__malloc_lock
                0x00004590       0x10 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
                0x00004590                __malloc_lock
 .text.__malloc_unlock
                0x000045a0       0x10 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
                0x000045a0                __malloc_unlock
 .text.__retarget_lock_acquire_recursive
                0x000045b0        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                0x000045b0                __retarget_lock_acquire_recursive
 .text.__retarget_lock_release_recursive
                0x000045b2        0x2 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                0x000045b2                __retarget_lock_release_recursive
 .text._sbrk    0x000045b4       0x1c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
                0x000045b4                _sbrk
 *(.init)
 .init          0x000045d0        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
                0x000045d0                _init
 .init          0x000045d4        0x8 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o
 *(.fini)
 .fini          0x000045dc        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
                0x000045dc                _fini
 .fini          0x000045e0        0x8 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o
 *crtbegin.o(.ctors)
 *crtbegin?.o(.ctors)
 *(EXCLUDE_FILE(*crtend.o *crtend?.o) .ctors)
 *(SORT_BY_NAME(.ctors.*))
 *(.ctors)
 *crtbegin.o(.dtors)
 *crtbegin?.o(.dtors)
 *(EXCLUDE_FILE(*crtend.o *crtend?.o) .dtors)
 *(SORT_BY_NAME(.dtors.*))
 *(.dtors)
 *(.rodata*)
 .rodata.g_APinDescription
                0x000045e8      0x450 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x000045e8                g_APinDescription
 .rodata._ZL10sercomData
                0x00004a38       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .rodata._ZTV4Uart
                0x00004a68       0x34 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                0x00004a68                vtable for Uart
 .rodata._ZN14USBDeviceClass19handleStandardSetupER8USBSetup.str1.1
                0x00004a9c        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 *fill*         0x00004a9d        0x3 
 .rodata._ZTV26DoubleBufferedEPOutHandler
                0x00004aa0       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x00004aa0                vtable for DoubleBufferedEPOutHandler
 .rodata._ZL14STRING_PRODUCT
                0x00004ac0        0xb C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 *fill*         0x00004acb        0x1 
 .rodata._ZL15STRING_LANGUAGE
                0x00004acc        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .rodata._ZL19STRING_MANUFACTURER
                0x00004ad0        0x9 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .rodata._ZL21USB_DeviceDescriptorB
                0x00004ad9       0x12 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 *fill*         0x00004aeb        0x1 
 .rodata._ZTV7Serial_
                0x00004aec       0x24 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x00004aec                vtable for Serial_
 *(.eh_frame*)
 .eh_frame      0x00004b10        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
 .eh_frame      0x00004b10        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtend.o

.glue_7         0x00004b14        0x0
 .glue_7        0x00004b14        0x0 linker stubs

.glue_7t        0x00004b14        0x0
 .glue_7t       0x00004b14        0x0 linker stubs

.vfp11_veneer   0x00004b14        0x0
 .vfp11_veneer  0x00004b14        0x0 linker stubs

.v4_bx          0x00004b14        0x0
 .v4_bx         0x00004b14        0x0 linker stubs

.iplt           0x00004b14        0x0
 .iplt          0x00004b14        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o

.rel.dyn        0x00004b14        0x0
 .rel.iplt      0x00004b14        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o

.ARM.extab
 *(.ARM.extab* .gnu.linkonce.armextab.*)
                0x00004b14                __exidx_start = .

.ARM.exidx
 *(.ARM.exidx* .gnu.linkonce.armexidx.*)
                0x00004b14                __exidx_end = .
                0x00004b14                __etext = .

.data           0x20000000      0x100 load address 0x00004b14
                0x20000000                __data_start__ = .
 *(vtable)
 *(.data*)
 .data.SystemCoreClock
                0x20000000        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                0x20000000                SystemCoreClock
 .data._ZL5ticks
                0x20000004        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .data.EndPoints
                0x20000008       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20000008                EndPoints
 .data._ZL10breakValue
                0x20000030        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .data._ZL12_usbLineInfo
                0x20000034        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .data._ZL13_cdcInterface
                0x2000003c       0x42 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 *fill*         0x2000007e        0x2 
 .data._serialPeek
                0x20000080        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x20000080                _serialPeek
 .data._impure_ptr
                0x20000084        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
                0x20000084                _impure_ptr
 .data.impure_data
                0x20000088       0x60 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
                0x200000e8                . = ALIGN (0x4)
                0x200000e8                PROVIDE (__preinit_array_start = .)
 *(.preinit_array)
                0x200000e8                PROVIDE (__preinit_array_end = .)
                0x200000e8                . = ALIGN (0x4)
                0x200000e8                PROVIDE (__init_array_start = .)
 *(SORT_BY_NAME(.init_array.*))
 *(.init_array)
 .init_array    0x200000e8        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
 .init_array    0x200000ec        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .init_array    0x200000f0        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .init_array    0x200000f4        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .init_array    0x200000f8        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x200000fc                PROVIDE (__init_array_end = .)
                0x200000fc                . = ALIGN (0x4)
                [!provide]                PROVIDE (__fini_array_start = .)
 *(SORT_BY_NAME(.fini_array.*))
 *(.fini_array)
 .fini_array    0x200000fc        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
                [!provide]                PROVIDE (__fini_array_end = .)
 *(.jcr*)
                0x20000100                . = ALIGN (0x10)
                0x20000100                __data_end__ = .

.igot.plt       0x20000100        0x0 load address 0x00004c14
 .igot.plt      0x20000100        0x0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o

.bss            0x20000100     0x4f3c load address 0x00004c14
                0x20000100                . = ALIGN (0x4)
                0x20000100                __bss_start__ = .
 *(.bss*)
 .bss           0x20000100       0x1c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
 .bss.ledState  0x2000011c        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x2000011c                ledState
 *fill*         0x2000011d        0x3 
 .bss.rpiUART0  0x20000120      0x23c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x20000120                rpiUART0
 .bss.rpiUART5  0x2000035c      0x23c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x2000035c                rpiUART5
 .bss.uartBuffer
                0x20000598     0x400c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                0x20000598                uartBuffer
 .bss.Serial1   0x200045a4      0x23c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x200045a4                Serial1
 .bss.Serial5   0x200047e0      0x23c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x200047e0                Serial5
 .bss.sercom0   0x20004a1c        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x20004a1c                sercom0
 .bss.sercom1   0x20004a20        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x20004a20                sercom1
 .bss.sercom2   0x20004a24        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x20004a24                sercom2
 .bss.sercom3   0x20004a28        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x20004a28                sercom3
 .bss.sercom4   0x20004a2c        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x20004a2c                sercom4
 .bss.sercom5   0x20004a30        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                0x20004a30                sercom5
 .bss.usb_isr   0x20004a34        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .bss._ulTickCount
                0x20004a38        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .bss.USBDevice
                0x20004a3c        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004a3c                USBDevice
 *fill*         0x20004a3d        0x3 
 .bss._ZL10epHandlers
                0x20004a40       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._ZL10rxLEDPulse
                0x20004a5c        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._ZL10txLEDPulse
                0x20004a5d        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._ZL14isEndpointHalt
                0x20004a5e        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._ZL20LastTransmitTimedOut
                0x20004a5f        0x7 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._ZL21isRemoteWakeUpEnabled
                0x20004a66        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 *fill*         0x20004a67        0x1 
 .bss._ZL22udd_ep_in_cache_buffer
                0x20004a68      0x1c0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._ZL23udd_ep_out_cache_buffer
                0x20004c28      0x1c0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .bss._dry_run  0x20004de8        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004de8                _dry_run
 .bss._pack_buffer
                0x20004de9      0x100 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004de9                _pack_buffer
 .bss._pack_message
                0x20004ee9        0x1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004ee9                _pack_message
 .bss._pack_size
                0x20004eea        0x2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004eea                _pack_size
 .bss._usbConfiguration
                0x20004eec        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004eec                _usbConfiguration
 .bss._usbSetInterface
                0x20004ef0        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004ef0                _usbSetInterface
 .bss.usbd      0x20004ef4      0x104 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                0x20004ef4                usbd
 .bss.Serial    0x20004ff8       0x1c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                0x20004ff8                Serial
 .bss._ZGVZ12PluggableUSBvE3obj
                0x20005014        0x4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .bss._ZZ12PluggableUSBvE3obj
                0x20005018        0x8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .bss.__malloc_free_list
                0x20005020        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                0x20005020                __malloc_free_list
 .bss.__malloc_sbrk_start
                0x20005024        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                0x20005024                __malloc_sbrk_start
 .bss.heap_end.4144
                0x20005028        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
 *(COMMON)
 COMMON         0x2000502c        0x4 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
                0x2000502c                errno
 COMMON         0x20005030        0x9 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                0x20005030                __lock___atexit_recursive_mutex
                0x20005031                __lock___arc4random_mutex
                0x20005032                __lock___env_recursive_mutex
                0x20005033                __lock___sinit_recursive_mutex
                0x20005034                __lock___malloc_recursive_mutex
                0x20005035                __lock___at_quick_exit_mutex
                0x20005036                __lock___dd_hash_mutex
                0x20005037                __lock___tz_mutex
                0x20005038                __lock___sfp_recursive_mutex
                0x2000503c                . = ALIGN (0x4)
 *fill*         0x20005039        0x3 
                0x2000503c                __bss_end__ = .

.heap           0x2000503c        0x0
                0x2000503c                __end__ = .
                0x2000503c                PROVIDE (end = .)
 *(.heap*)
                0x2000503c                __HeapLimit = .

.stack_dummy    0x2000503c        0x0
 *(.stack*)
                0x20008000                __StackTop = (ORIGIN (RAM) + LENGTH (RAM))
                0x20008000                __StackLimit = (__StackTop - SIZEOF (.stack_dummy))
                0x20008000                PROVIDE (__stack = __StackTop)
                0x20007fff                __ram_end__ = ((ORIGIN (RAM) + LENGTH (RAM)) - 0x1)
                0x00000001                ASSERT ((__StackLimit >= __HeapLimit), region RAM overflowed with stack)
OUTPUT(C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/mux_rpi.ino.elf elf32-littlearm)

.ARM.attributes
                0x00000000       0x28
 .ARM.attributes
                0x00000000       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
 .ARM.attributes
                0x0000001e       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
 .ARM.attributes
                0x0000004a       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .ARM.attributes
                0x00000076       0x32 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .ARM.attributes
                0x000000a8       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .ARM.attributes
                0x000000d4       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .ARM.attributes
                0x00000100       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .ARM.attributes
                0x0000012c       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .ARM.attributes
                0x00000158       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .ARM.attributes
                0x00000184       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .ARM.attributes
                0x000001b0       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .ARM.attributes
                0x000001dc       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .ARM.attributes
                0x00000208       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .ARM.attributes
                0x00000234       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .ARM.attributes
                0x00000260       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .ARM.attributes
                0x0000028c       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .ARM.attributes
                0x000002b8       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .ARM.attributes
                0x000002e4       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .ARM.attributes
                0x00000310       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .ARM.attributes
                0x0000033c       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .ARM.attributes
                0x00000368       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .ARM.attributes
                0x00000394       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
 .ARM.attributes
                0x000003c0       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_uqi.o)
 .ARM.attributes
                0x000003de       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
 .ARM.attributes
                0x000003fc       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
 .ARM.attributes
                0x0000041a       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
 .ARM.attributes
                0x00000446       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
 .ARM.attributes
                0x00000472       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
 .ARM.attributes
                0x0000049e       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
 .ARM.attributes
                0x000004ca       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
 .ARM.attributes
                0x000004f6       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
 .ARM.attributes
                0x00000522       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
 .ARM.attributes
                0x0000054e       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
 .ARM.attributes
                0x0000057a       0x1c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-strlen.o)
 .ARM.attributes
                0x00000596       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
 .ARM.attributes
                0x000005c2       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .ARM.attributes
                0x000005ee       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .ARM.attributes
                0x0000061a       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
 .ARM.attributes
                0x00000646       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtend.o
 .ARM.attributes
                0x00000672       0x1e c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtn.o

.comment        0x00000000       0xf7
 .comment       0x00000000       0x79 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                                 0x7a (size before relaxing)
 .comment       0x00000079       0x7e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                 0x7f (size before relaxing)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .comment       0x000000f7       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_info     0x00000000    0x702d1
 .debug_info    0x00000000     0x8285 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_info    0x00008285     0x6520 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_info    0x0000e7a5     0x121b C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_info    0x0000f9c0     0x14c5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_info    0x00010e85       0x67 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .debug_info    0x00010eec     0x3863 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_info    0x0001474f     0x307e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_info    0x000177cd     0x5505 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_info    0x0001ccd2     0x19bd C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_info    0x0001e68f     0x194b C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_info    0x0001ffda     0x6ecd C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .debug_info    0x00026ea7     0x8091 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_info    0x0002ef38     0x9cbe C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_info    0x00038bf6     0x68d4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .debug_info    0x0003f4ca     0x91a9 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_info    0x00048673     0xe9f7 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_info    0x0005706a     0x1111 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_info    0x0005817b     0x8e13 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_info    0x00060f8e     0x6d7d C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_info    0x00067d0b     0x85c6 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_abbrev   0x00000000     0x7b40
 .debug_abbrev  0x00000000      0x8ed C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_abbrev  0x000008ed      0x541 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_abbrev  0x00000e2e      0x303 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_abbrev  0x00001131      0x33a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_abbrev  0x0000146b       0x4d C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .debug_abbrev  0x000014b8      0x2f7 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_abbrev  0x000017af      0x3e8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_abbrev  0x00001b97      0x554 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_abbrev  0x000020eb      0x389 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_abbrev  0x00002474      0x351 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_abbrev  0x000027c5      0x750 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .debug_abbrev  0x00002f15      0x974 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_abbrev  0x00003889      0xa49 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_abbrev  0x000042d2      0x683 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .debug_abbrev  0x00004955      0x9ae C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_abbrev  0x00005303      0xcf4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_abbrev  0x00005ff7      0x350 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_abbrev  0x00006347      0x9bf C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_abbrev  0x00006d06      0x778 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_abbrev  0x0000747e      0x6c2 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_loc      0x00000000     0x7886
 .debug_loc     0x00000000      0x102 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_loc     0x00000102       0x2a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_loc     0x0000012c       0xa5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_loc     0x000001d1      0x12a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_loc     0x000002fb       0x47 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_loc     0x00000342       0xd9 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_loc     0x0000041b      0x51c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_loc     0x00000937      0x13e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_loc     0x00000a75      0x14e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_loc     0x00000bc3      0xe80 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_loc     0x00001a43      0xc6d C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_loc     0x000026b0     0x1755 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_loc     0x00003e05     0x3092 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_loc     0x00006e97       0x4a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_loc     0x00006ee1      0x657 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_loc     0x00007538      0x295 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_loc     0x000077cd       0xb9 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_aranges  0x00000000      0x8e8
 .debug_aranges
                0x00000000       0x70 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_aranges
                0x00000070       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_aranges
                0x000000a0       0x40 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_aranges
                0x000000e0       0x38 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_aranges
                0x00000118       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .debug_aranges
                0x00000148       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_aranges
                0x00000168       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_aranges
                0x00000188       0x40 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_aranges
                0x000001c8       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_aranges
                0x000001f8       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_aranges
                0x00000218       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .debug_aranges
                0x00000248      0x200 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_aranges
                0x00000448       0xb0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_aranges
                0x000004f8       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .debug_aranges
                0x00000520      0x108 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_aranges
                0x00000628      0x180 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_aranges
                0x000007a8       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_aranges
                0x000007d0       0xa0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_aranges
                0x00000870       0x50 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_aranges
                0x000008c0       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_ranges   0x00000000     0x16b8
 .debug_ranges  0x00000000       0xd0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_ranges  0x000000d0       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_ranges  0x000000f0       0x30 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_ranges  0x00000120       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_ranges  0x00000148       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .debug_ranges  0x00000168       0x10 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_ranges  0x00000178       0x80 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_ranges  0x000001f8       0xd8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_ranges  0x000002d0       0x20 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_ranges  0x000002f0       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_ranges  0x00000318       0x50 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .debug_ranges  0x00000368      0x320 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_ranges  0x00000688      0x260 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_ranges  0x000008e8       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .debug_ranges  0x00000900      0x208 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_ranges  0x00000b08      0x9f8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_ranges  0x00001500       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_ranges  0x00001518      0x128 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_ranges  0x00001640       0x60 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_ranges  0x000016a0       0x18 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_line     0x00000000     0xd6a1
 .debug_line    0x00000000      0xc05 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_line    0x00000c05      0x62c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_line    0x00001231      0x4b1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_line    0x000016e2      0x6f5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_line    0x00001dd7       0xd5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .debug_line    0x00001eac      0x71a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_line    0x000025c6      0x769 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_line    0x00002d2f      0xc0e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_line    0x0000393d      0x63f C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_line    0x00003f7c      0x5d5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_line    0x00004551      0x910 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .debug_line    0x00004e61     0x16eb C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_line    0x0000654c      0xfd7 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_line    0x00007523      0x7e1 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .debug_line    0x00007d04      0xf59 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_line    0x00008c5d     0x28aa C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_line    0x0000b507      0x431 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_line    0x0000b938      0xb7b C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_line    0x0000c4b3      0x9e3 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_line    0x0000ce96      0x80b C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)

.debug_str      0x00000000     0xa8e5
 .debug_str     0x00000000     0x421e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                               0x4cc5 (size before relaxing)
 .debug_str     0x0000421e      0x74d C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                               0x3791 (size before relaxing)
 .debug_str     0x0000496b      0x4dd C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                                0xfe6 (size before relaxing)
 .debug_str     0x00004e48       0xcb C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                                0xee8 (size before relaxing)
 .debug_str     0x00004f13       0x7a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
                                0x189 (size before relaxing)
 .debug_str     0x00004f8d      0x832 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
                               0x1723 (size before relaxing)
 .debug_str     0x000057bf      0x205 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                               0x181d (size before relaxing)
 .debug_str     0x000059c4      0x16f C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                               0x1c7c (size before relaxing)
 .debug_str     0x00005b33      0x112 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                                0xfee (size before relaxing)
 .debug_str     0x00005c45       0x7e C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
                                0xfdb (size before relaxing)
 .debug_str     0x00005cc3      0x1a5 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                               0x4301 (size before relaxing)
 .debug_str     0x00005e68      0x228 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                               0x45b0 (size before relaxing)
 .debug_str     0x00006090     0x171a C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                               0x5bd2 (size before relaxing)
 .debug_str     0x000077aa       0xb6 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                               0x40c9 (size before relaxing)
 .debug_str     0x00007860      0x41b C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
                               0x4fdf (size before relaxing)
 .debug_str     0x00007c7b     0x2507 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                               0x7300 (size before relaxing)
 .debug_str     0x0000a182       0x93 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                                0x817 (size before relaxing)
 .debug_str     0x0000a215      0x581 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                               0x58fb (size before relaxing)
 .debug_str     0x0000a796       0x97 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                               0x4359 (size before relaxing)
 .debug_str     0x0000a82d       0xb8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                               0x5bdf (size before relaxing)

.debug_frame    0x00000000     0x183c
 .debug_frame   0x00000000      0x100 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
 .debug_frame   0x00000100       0x64 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
 .debug_frame   0x00000164       0x78 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
 .debug_frame   0x000001dc       0x78 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
 .debug_frame   0x00000254       0x40 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
 .debug_frame   0x00000294       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
 .debug_frame   0x000002c0       0x28 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
 .debug_frame   0x000002e8       0x80 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
 .debug_frame   0x00000368       0x60 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
 .debug_frame   0x000003c8       0x2c C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
 .debug_frame   0x000003f4       0x48 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
 .debug_frame   0x0000043c      0x4a0 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
 .debug_frame   0x000008dc      0x1c4 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
 .debug_frame   0x00000aa0       0x38 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
 .debug_frame   0x00000ad8      0x334 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
 .debug_frame   0x00000e0c      0x474 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
 .debug_frame   0x00001280       0x70 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
 .debug_frame   0x000012f0      0x188 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
 .debug_frame   0x00001478       0xc8 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
 .debug_frame   0x00001540       0x48 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
 .debug_frame   0x00001588       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
 .debug_frame   0x000015a8       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
 .debug_frame   0x000015d4       0x40 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
 .debug_frame   0x00001614       0x28 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
 .debug_frame   0x0000163c       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
 .debug_frame   0x0000165c       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
 .debug_frame   0x00001688       0x30 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
 .debug_frame   0x000016b8       0x2c c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
 .debug_frame   0x000016e4       0x40 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
 .debug_frame   0x00001724       0x48 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
 .debug_frame   0x0000176c       0xb0 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
 .debug_frame   0x0000181c       0x20 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)

Cross Reference Table

Symbol                                            File
AC_Handler                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
ADC_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
CDC_GetInterface(unsigned char*)                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
CDC_Setup(USBSetup&)                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DAC_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
DMAC_Handler                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
DoubleBufferedEPOutHandler::available() const     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::handleEndpoint()      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::init()                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::recv(void*, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::release()             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler() C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler() C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
DoubleBufferedEPOutHandler::~DoubleBufferedEPOutHandler() C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
Dummy_Handler                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
EIC_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
EVSYS_Handler                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
EndPoints                                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
HardFault_Handler                                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
I2S_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
NMI_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
NVMCTRL_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
PM_Handler                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
PTC_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
PendSV_Handler                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
PluggableUSB()                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
PluggableUSB_::PluggableUSB_()                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
PluggableUSB_::PluggableUSB_()                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
PluggableUSB_::getDescriptor(USBSetup&)           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
PluggableUSB_::getInterface(unsigned char*)       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
PluggableUSB_::getShortName(char*)                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
PluggableUSB_::plug(PluggableUSBModule*)          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
PluggableUSB_::setup(USBSetup&)                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(PluggableUSB.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
Print::availableForWrite()                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::flush()                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(Printable const&)                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(String const&)                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(__FlashStringHelper const*)          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(char const*)                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(char)                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(double, int)                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(int, int)                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(long, int)                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(unsigned char, int)                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(unsigned int, int)                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::print(unsigned long, int)                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::printFloat(double, unsigned char)          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::printNumber(unsigned long, unsigned char)  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::printf(char const*, ...)                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println()                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(Printable const&)                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(String const&)                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(__FlashStringHelper const*)        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(char const*)                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(char)                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(double, int)                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(int, int)                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(long, int)                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(unsigned char, int)                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(unsigned int, int)                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::println(unsigned long, int)                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::write(char const*)                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
Print::write(unsigned char const*, unsigned int)  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
RTC_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
Reset_Handler                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
RingBufferN<256>::RingBufferN()                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
RingBufferN<256>::RingBufferN()                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
RingBufferN<256>::available()                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
RingBufferN<256>::availableForStore()             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM0_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
SERCOM1_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
SERCOM2_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
SERCOM3_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
SERCOM4_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
SERCOM5_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
SERCOM::SERCOM(Sercom*)                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::SERCOM(Sercom*)                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
SERCOM::acknowledgeUARTError()                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::availableDataUART()                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::availableWIRE()                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::calculateBaudrateSynchronous(unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::clearFrameErrorUART()                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::clearStatusUART()                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::disableDataRegisterEmptyInterruptUART()   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::disableSPI()                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::disableWIRE()                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::enableDataRegisterEmptyInterruptUART()    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::enableSPI()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::enableUART()                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::enableWIRE()                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::flushUART()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::getDataOrderSPI()                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::getSercomIndex()                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::initClockNVIC()                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::initFrame(SercomUartCharSize, SercomDataOrder, SercomParityMode, SercomNumberStopBit) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::initMasterWIRE(unsigned long)             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::initPads(SercomUartTXPad, SercomRXPad)    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::initSPI(SercomSpiTXPad, SercomRXPad, SercomSpiCharSize, SercomDataOrder) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::initSPIClock(SercomSpiClockMode, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::initSlaveWIRE(unsigned char, bool)        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::initUART(SercomUartMode, SercomUartSampleRate, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::isAddressMatch()                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isArbLostWIRE()                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isBufferOverflowErrorSPI()                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isBufferOverflowErrorUART()               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isBusBusyWIRE()                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isBusIdleWIRE()                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isBusOwnerWIRE()                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isBusUnknownWIRE()                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isDataReadyWIRE()                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isDataRegisterEmptySPI()                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isDataRegisterEmptyUART()                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::isFrameErrorUART()                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::isMasterReadOperationWIRE()               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isMasterWIRE()                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isParityErrorUART()                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isRXNackReceivedWIRE()                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isRestartDetectedWIRE()                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isSlaveWIRE()                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isStopDetectedWIRE()                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::isUARTError()                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::prepareAckBitWIRE()                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::prepareCommandBitsWire(unsigned char)     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::prepareNackBitWIRE()                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::readDataUART()                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::readDataWIRE()                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::resetSPI()                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::resetUART()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SERCOM::resetWIRE()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::sendDataMasterWIRE(unsigned char)         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::sendDataSlaveWIRE(unsigned char)          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::setBaudrateSPI(unsigned char)             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::setClockModeSPI(SercomSpiClockMode)       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::setDataOrderSPI(SercomDataOrder)          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::startTransmissionWIRE(unsigned char, SercomWireReadWriteFlag) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::transferDataSPI(unsigned char)            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
SERCOM::writeDataUART(unsigned char)              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
SVC_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
SYSCTRL_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
Serial                                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial1                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
Serial5                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
Serial_::available()                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::availableForWrite()                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::begin(unsigned long)                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::begin(unsigned long, unsigned char)      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::end()                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::flush()                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::operator bool()                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::peek()                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::read()                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::readBytes(char*, unsigned int)           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::write(unsigned char const*, unsigned int) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
Serial_::write(unsigned char)                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
SysTick_DefaultHandler                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
SysTick_Handler                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
SystemCoreClock                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
SystemInit                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(startup.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TC3_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TC4_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TC5_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TC6_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TC7_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TCC0_Handler                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TCC1_Handler                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
TCC2_Handler                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
UDD_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDevice                                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
USBDeviceClass::ISRHandler()                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::SendInterfaces(unsigned long*)    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::armRecv(unsigned long)            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::armRecvCtrlOUT(unsigned long)     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::armSend(unsigned long, void const*, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::attach()                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
USBDeviceClass::available(unsigned long)          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::configured()                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::connected()                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::detach()                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::end()                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::flush(unsigned long)              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::handleClassInterfaceSetup(USBSetup&) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::handleEndpoint(unsigned char)     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::handleStandardSetup(USBSetup&)    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::init()                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
USBDeviceClass::initEP(unsigned long, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::initEndpoints()                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::packMessages(bool)                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::recv(unsigned long)               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::recv(unsigned long, void*, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::recvControl(void*, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::send(unsigned long, void const*, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::sendConfiguration(unsigned long)  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::sendControl(void const*, unsigned long) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
USBDeviceClass::sendDescriptor(USBSetup&)         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::sendStringDescriptor(unsigned char const*, unsigned char) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::sendZlp(unsigned long)            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::setAddress(unsigned long)         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::setHandler(unsigned long, EPHandler*) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::stall(unsigned long)              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDeviceClass::standby()                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDevice_SAMD21G18x::calibrate()                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USBDevice_SAMD21G18x::reset()                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
USB_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
USB_SetHandler                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
Uart::IrqHandler()                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad, unsigned char, unsigned char) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::Uart(SERCOM*, unsigned char, unsigned char, SercomRXPad, SercomUartTXPad, unsigned char, unsigned char) C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::available()                                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::availableForWrite()                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::begin(unsigned long)                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::begin(unsigned long, unsigned short)        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::end()                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::extractCharSize(unsigned short)             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::extractNbStopBit(unsigned short)            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::extractParity(unsigned short)               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::flush()                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::operator bool()                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::peek()                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::read()                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
Uart::write(unsigned char)                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
WDT_Handler                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
_CDC_GetInterface()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
_CDC_GetInterfaceLength()                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
__Guard::__Guard()                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
__Guard::__Guard()                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
__Guard::~__Guard()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
__Guard::~__Guard()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
__StackTop                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
__aeabi_cdcmpeq                                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__aeabi_cdcmple                                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__aeabi_cdrcmple                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__aeabi_d2iz                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(fixdfsi.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
__aeabi_d2uiz                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dadd                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dcmpeq                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__aeabi_dcmpge                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
__aeabi_dcmpgt                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dcmple                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dcmplt                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dcmpun                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(unorddf2.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_ddiv                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dmul                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_dsub                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_idiv                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
__aeabi_idiv0                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
__aeabi_idivmod                                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
__aeabi_ldiv0                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_dvmd_tls.o)
__aeabi_ui2d                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__aeabi_uidiv                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SERCOM.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
__aeabi_uidivmod                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__bss_end__                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
__bss_start__                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
__call_exitprocs                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
__clzsi2                                          c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_clzsi2.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(floatunsidf.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(subdf3.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(muldf3.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(divdf3.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(adddf3.o)
__cxa_deleted_virtual                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
__cxa_pure_virtual                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(abi.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
__data_end__                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
__data_start__                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
__deregister_frame_info                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
__divsi3                                          c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_divsi3.o)
__dso_handle                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
__eqdf2                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__etext                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
__fixunsdfsi                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_fixunsdfsi.o)
__gedf2                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__gnu_thumb1_case_shi                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_shi.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
__gnu_thumb1_case_uqi                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_thumb1_case_uqi.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
__gtdf2                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(gedf2.o)
__init_array_end                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
__init_array_start                                c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
__ledf2                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_arm_cmpdf2.o)
__libc_fini_array                                 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
__libc_init_array                                 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
__lock___arc4random_mutex                         c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___at_quick_exit_mutex                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___atexit_recursive_mutex                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___dd_hash_mutex                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___env_recursive_mutex                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___malloc_recursive_mutex                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
__lock___sfp_recursive_mutex                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___sinit_recursive_mutex                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__lock___tz_mutex                                 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__ltdf2                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(ledf2.o)
__malloc_free_list                                c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
__malloc_lock                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
__malloc_sbrk_start                               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
__malloc_unlock                                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
__nedf2                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(eqdf2.o)
__preinit_array_end                               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
__preinit_array_start                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
__register_frame_info                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crtbegin.o
__retarget_lock_acquire                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_acquire_recursive                 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
__retarget_lock_close                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_close_recursive                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_init                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_init_recursive                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_release                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_release_recursive                 c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-mlock.o)
__retarget_lock_try_acquire                       c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__retarget_lock_try_acquire_recursive             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-lock.o)
__sf_fake_stderr                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
__sf_fake_stdin                                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
__sf_fake_stdout                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
__ssprint_r                                       c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
__ssputs_r                                        c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
__stack                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
__text_start__                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
__udivsi3                                         c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp\libgcc.a(_udivsi3.o)
_dry_run                                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
_exit                                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(_exit.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
_fini                                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
_free_r                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-freer.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
_global_impure_ptr                                c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
_impure_ptr                                       c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-impure.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
_init                                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/thumb/v6-m/nofp/crti.o
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-init.o)
_mainCRTStartup                                   c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
_malloc_r                                         c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
_malloc_usable_size_r                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-msizer.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
_pack_buffer                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
_pack_message                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
_pack_size                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
_printf_common                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
_printf_float                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
_printf_i                                         c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
_realloc_r                                        c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
_reclaim_reent                                    c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
_sbrk                                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
_sbrk_r                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-mallocr.o)
_serialPeek                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
_start                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
_svfiprintf_r                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
_svfprintf_r                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
_usbConfiguration                                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
_usbSetInterface                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
_vsniprintf_r                                     c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
_vsnprintf_r                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
analogRead                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
analogReadResolution                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
analogReference                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
analogWrite                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
analogWriteResolution                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
atexit                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
cancelReset                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
cleanup_glue                                      c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
delay                                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
digitalRead                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
digitalWrite                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
end                                               c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libnosys.a(sbrk.o)
errno                                             c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-reent.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-sbrkr.o)
exception_table                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
exit                                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-exit.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
free                                              c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
g_APinDescription                                 C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
g_apTCInstances                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
hardware_init_hook                                c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
init                                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
initVariant()                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
initiateReset                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
ledState                                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
loop                                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
main                                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
malloc                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-malloc.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
memchr                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memchr-stub.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-vfprintf_i.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
memcpy                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memcpy-stub.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-reallocr.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
memmove                                           c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memmove.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-nano-svfprintf.o)
memset                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-memset.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(SAMD21_USBDevice.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                                                  c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
micros                                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
millis                                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
operator delete(void*)                            C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
operator delete[](void*)                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
operator new(unsigned int)                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
operator new[](unsigned int)                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(new.cpp.o)
pendSVHook                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
pinMode                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_digital.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
pinPeripheral                                     C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_private.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(wiring_analog.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
rpiUART0                                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
rpiUART5                                          C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
sercom0                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
sercom1                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
sercom2                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
sercom3                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
sercom4                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
sercom5                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\core\variant.cpp.o
serialEventRun()                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
setup                                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
software_init_hook                                c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp/crt0.o
strlen                                            c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-strlen.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
svcHook                                           C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
sysTickHook                                       C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(cortex_handlers.c.o)
tickReset                                         C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Reset.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
timerConfigure(int)                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
timerDisable()                                    C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
timerIsSyncing()                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
timerReset()                                      C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
timerStartCounter()                               C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
uartBuffer                                        C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D\sketch\mux_rpi.ino.cpp.o
usbd                                              C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
vsniprintf                                        c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
vsnprintf                                         c:/users/mcros/appdata/local/arduino15/packages/adafruit/tools/arm-none-eabi-gcc/9-2019q4/bin/../lib/gcc/arm-none-eabi/9.2.1/../../../../arm-none-eabi/lib/thumb/v6-m/nofp\libc_nano.a(lib_a-vsnprintf.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
vtable for DoubleBufferedEPOutHandler             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(USBCore.cpp.o)
vtable for Print                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Print.cpp.o)
vtable for Serial_                                C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(CDC.cpp.o)
vtable for Uart                                   C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(Uart.cpp.o)
yield                                             C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(hooks.c.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(main.cpp.o)
                                                  C:\Users\mcros\AppData\Local\Temp\arduino-sketch-5058F1AF8388633F609CADB75A75DC9D/..\arduino-core-cache\core_adafruit_samd_adafruit_feather_m0_ab58fdfd23df71d37e67d375b2dd6b7c.a(delay.c.o)
